## EdgeIQ

Welcome to EdgeIQ! This documentation provides brief instructions on how to install and configure EdgeIQ on your
infrastructure.
For a detailed guide, refer to the [EdgeIQ documentation](https://docs.behavure.ai/).

## Quick Start on Linux (x86_64)

To quickly install EdgeIQ on a Linux system, follow the steps below:

1. Download the latest binary the links in the documentation or the main website.
2. Extract the binary to a directory of your choice.

> **Note:** The binary is a `xz` compressed tarball. You can extract it using the following command:
> ```sh
> tar -xxf edgeiq-x86_64-unknown-linux-gnu.tar.xz
> ```

3. Copy the binary to a directory in your `PATH` environment variable.

> **Note:** You may copy the binary to the `/usr/local/bin`  which normally is a directory in your `PATH`
> environment variable using the following command:
> ```sh
> sudo cp edgeiq /usr/local/bin
> ```

4. Run the following command to start the EdgeIQ Server:

```sh
edgeiq run server
```

> **Note:** The Server will start on `localhost:3000` by default. You can access the Server via a browser at
> `http://localhost:3000`.
> You will need the randomly generated password for the default `admin` which is displayed on the console when you start
> the Server.

For more detailed instructions and other platforms refer to the [EdgeIQ documentation](https://docs.edgeIQ.com/).



